1. What is the minimum weight for any sling load to fly?
2. What is the hook capacity of the UH-60L/M?
3. What are the factors of in-flight stability?
4. What reference material covers single point rigging procedures?
5. What is the rank requirement for a qualified sling load inspector?
6. What is the diameter of the 10k apex pin portion?
7. What is the primary lift point on the 500 gallon fuel blivet?
8. How often should you inspect sling load equipment?
9. What is the least preferred method of improving in-flight stability?
10. What are the phases of a sling load operation?
11. What is the rated capacity of the small cargo hook reach pendant?
12. What is the maximum weight of a single fuel blivet?
13. What is the rated capacity of a single 25k sling leg?
14. What is the hook capacity of the fore or aft cargo hooks individually on a CH-47?
15. What is the weight of a complete 10k sling set?
16. What is the weight of a complete 25k sling set?
17. What is the link count for the 5K cargo net when utilizing a 10K Sling leg?
18. How many breakaways are required on the cargo net?
19. How can the large clevis be used?
20. Where can you find DA Form 7382?
21. When a link count is 10 or more, how will excess links will be secured?
22. What is the rated capacity of the black load binder?
23. What are the dimensions of the 5K cargo net?
24. What is the link count for the single fuel blivet?
25. What is the rule of thumb when inspecting the stitching on the A-22 cargo bag?
26. What is the maximum weight of the A-22 cargo bag?
27. What is the purpose of the static discharge wand?
28. What is the rated capacity of ¼ inch cotton webbing?
29. What is the rated capacity of the small screw pin clevis?
30. What classification of sling load has flown for years without incident?
31. What unit is responsible for selecting, preparing, and controlling the PZ?
32. What reference material covers dual point rigging procedures?
33. A qualified sling load inspector must be in the grade of E-4 or above and must be a graduate of which school?
34. What reference material covers basic operations and equipment?
35. How many links are on a 25k lifting chain?
36. How is the proper drag surface achieved?
37. What is the rated capacity of the medium clevis?
38. What are the dimensions of the 10k cargo net?
39. What is the link count for the A-22 cargo bag?
40. What is the load bearing zone size of the 10k cargo net?
41. What is the proper uniform for ground crew members conducting sling load operations?
42. What is the hook capacity of the UH-60A?
43. What is the hook sequence for the cargo net?
44. What is the rated capacity of 7/16 inch nylon rope?
45. How much of the load must be inside the load bearing zone of the 5k and 10k cargo nets?
46. What unit is responsible for providing assistance in the recovery and return of all sling load equipment?
47. What is the rated capacity of the CGU-1B?
48. What is the rated capacity of the large clevis?
49. How many breakaways are required on the M149A2 water trailer?
50. What can be used as breakaway material?
51. How will the excess lacing ropes be secured on the A-22 cargo bag?
52. What is the hook capacity of the center cargo hook?
53. What is the empty weight of the M1151 up armored HMMWV?
54. What is the rated capacity of the type IV connector link?
55. What is the link count for the M149A2 water trailer?
56. What is the rated capacity of type III nylon?
57. What is the rated capacity of the 25k apex?
58. What is the average empty weight of a single fuel blivet?
59. What is the rated capacity of ½ inch tubular nylon?
60. What is the rated capacity of the net apex fitting?
61. What is the rated capacity of a complete 10k sling set?
62. How many links are on a 10k lifting chain?
63. What is the purpose of the apex tether cord?
64. Who can release the cargo hook from inside the UH-60?
65. What is the rated capacity of the 10k apex?
66. What is the rated capacity of the large cargo hook reach pendant?
67. What is the rated capacity of 2” tape?
68. What is the rated capacity of the silver load binder?
69. What are the components of the type IV connector link?
70. What is the rated capacity for the Ariel delivery sling?
71. What is the maximum weight of four 500 gallon fuel blivets?
72. What manual covers basic operations and equipment?
73. Which cargo hook on the CH-47 cannot be released manually?
74. What is the ACL for the M1101 high mobility trailer?
75. What direction is the M149A2 water trailer flown?
76. What is the link count of the M1101 high mobility trailer with a 10k sling set?
77. What will render the Ariel delivery sling unserviceable?
78. What would you use to clean the metal portions of any sling set?
79. Can a UH-60 use a nylon point of attachment?
80. How would a CH-47 carry three single point of attachment loads that all have different weights?
81. Who is the approving authority for a unique load to fly?
82. What equipment is used to secure equipment in the back of vehicles and trailers?
83. What is the rated capacity of the 3/8 inch Hemp rope?
84. Where can the damage criteria chart for sling legs be found?
85. What material is the rope portion on sling legs?
86. Where can you find on how to make a field expedient static discharge wand?
87. How should the grounding rod be placed into the ground?
88. What are 5 ways to improve in flight stability?
89. Where do the three copies of DA Form 7382 go?
90. What must be removed when using a 25k sling set on a UH-60?